slacHeadeQC

# Leave Blank MFD NON-COMPLIANCE REPORT # 27498-63

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| PART NAME: | **ALIGNMENT PIN 2** | DATE: | **7/6/12** | | |
| PF/SA NO.: | **PF-380-545-30 R0** | INSPECTOR: | **K. CABAN** | | |
| WORK ORDER NO.: | **27498-63 & 27937-50** | ENGINEER: | **E. KRAFT** | EXT.: | **2061** |
| VENDOR | **MFD** | ROUTE TO: | **MTLFNSH** | | |

|  |  |
| --- | --- |
| Reason For Non-Compliance: | Action (**UAI,RWK,SCRP)** |
| \*\* NCR IS FOR BOTH MFD W/O#: 27498-63 & 27937-50 (QTY: 4 PER W/O)   1. ALL PARTS (8 TOTAL) tmpCAB2.tmp ARE UNDERSIZED. SEE ATTACHED PROFILE PLOTS FOR EACH PART. 2. PART #3 ONLY, SPHERICAL RADIUS NOMINAL SR .188 MEASURES .179, BUT SHAFT DIAMETER TOLERANCE IS .375 ± 0.020. |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Engineer Signature: |  | Date: |  |