NON-COMPLIANCE REPORT # 32739-0

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| PART NAME: | **SOCKETS, TOOLING BALL** | DATE: | **2/26/16** | | |
| PF/SA NO.: | **PF-444-316-76** | INSPECTOR: | **K. CABAN** | | |
| WORK ORDER NO.: | **32739-0** | ENGINEER: | **J. AMANN** | EXT.: | **4768** |
| VENDOR | **SWISS SCREW** | PLANNER: | **BILL** | | |

|  |  |
| --- | --- |
| **Reason for Non-Compliance:** | **Disposition (UAI, Rework, Scrap, Other):** |

1.  - Magnetic permeability measures between 1.060 to 1.179on  
   2X flat surfaces.