Procedures for Pitch Adapter Traces

1. Position such that Zero Center Hole is in the upper portion of the stage.

2. Align traces in Y

3. Zero center hole  X,Y,Z = 0

4. Measure # 4, 5, 6, 7, 15, 9

5. Zero trace 9

6. Measure 27, 14, 13, 12, 11, 10

7. Zero trace 10

8. Measure 26

9. Follow trace 10 to the left & zero 10.

10. Measure 25, 23, 24, 22, 21, 20, 18, 19

11. Shift Part such that Zero Center Hole is in the lower portion of the stage.

12. Align traces in Y

13. Zero center hole X, Y, Z = 0

14. Measure 1, 2, 3, 16, 17

