Avg of Runs 1-4, in which the power supply stayed on and the measurements were repeated.  

BL/I at 0.2 amps = 0.00960225 Tm/A +/- 2.602e-5.  Std/Avg = 0.0027.

Avg of Runs 5-7, in which the power supply was turned off then on and set using the recall 3 button sequence.  

BL/I at 0.2 amps  =0.0095903 +/- 4.236e-5. 

BL/I Avg Run 1-4 / BL/I Run 5-7 = 0.00960225/0.0095903  = 1.001246

Avg of Runs 9-11, in which the power supply was turned off then on and set to 2 or 5 amps then dialed recalled to 0.2.  

BL/I at 0.2 amps  =0.009607 +/- 1.539e-4.  

BL/I Run 9-11 / BL/I Avg Run 1-4 = 0.009607 /0.00960225 = 1.0005