SLAC Magnetic Measurements# Date: 06-14-2018# Time: 18:36:19#

0.5 1 1.5 2 2.5

Potentiometer (V) 10 12 14 16 18 20 22 24 26 28 30

Encoder (mm)

Upstream Potentiometer vs Encoder

Measurements

Linear Fit

0.5 1 1.5 2 2.5 Potentiometer (V)

-0.05

-0.04

-0.03

-0.02

-0.01 0 0.01

0.02

0.03

0.04

Residual (mm)

Upstream Linear Fit Residuals

0.5 1 1.5 2 2.5

Potentiometer (V) 10 12 14 16 18 20 22 24 26 28 30

Encoder (mm)

Upstream Potentiometer vs Encoder

Measurements

Third Order Fit

0.5 1 1.5 2 2.5 Potentiometer (V)

-0.02

-0.01

0

0.01

0.02

0.03

0.04

Residual (mm)

Upstream Third Order Fit Residuals

0.5 1 1.5 2 2.5

Potentiometer (V) 10 12 14 16 18 20 22 24 26 28 30

Encoder (mm)

Downstream Potentiometer vs Encoder

Measurements

Linear Fit

0.5 1 1.5 2 2.5 Potentiometer (V)

-0.08

-0.06

-0.04

-0.02

0

0.02

0.04

0.06

Residual (mm)

Downstream Linear Fit Residuals

0.5 1 1.5 2 2.5

Potentiometer (V) 10 12 14 16 18 20 22 24 26 28 30

Encoder (mm)

Downpstream Potentiometer vs Encoder

Measurements

Third Order Fit

0.5 1 1.5 2 2.5 Potentiometer (V)

-0.02

-0.015

-0.01

-0.005

0

0.005

0.01

0.015

Residual (mm)

Downstream Third Order Fit Residuals