Hall probe alignment.  

Hall element assumed to be at location defined by Active area: MMT/HMMT-6JXX page in Lakeshore Hall Probe Active Areas.pdf

X = 0. Hall element set to pole 1 mechanical center.
Y= 0  Hall element set to pole 1 mechanical center.
Z = 0 Hall element set to pole 1 incoming edge.