NON-COMPLIANCE REPORT # M-24857

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| PART NAME: | **PUMPOUT RING** | DATE: | **5/12/15** | | |
| PF/SA NO.: | **PF-700-931-44 R2** | INSPECTOR: | **K. CABAN** | | |
| WORK ORDER NO.: | **M-24857** | ENGINEER: | **HAASE** | EXT.: | **8612** |
| VENDOR | **KLY MACHINE SHOP** | ROUTE TO: |  | | |

|  |  |
| --- | --- |
| **Reason for Non-Compliance:** | **Disposition (UAI, Rework, Scrap, Other):** |

1.  measures 0.0041 – 0.0047 on SN 127, 128 & 132 only.
2.  of  measures 0.0025 - 0.0051 on SN 125, 126, 130, 134, 138 & 139 only.
3. +0.002/-0.000 measure undersized: 8.9970 – 8.9987 on all parts