NON-COMPLIANCE REPORT # 31787-54

|  |  |  |  |
| --- | --- | --- | --- |
| PART NAME: | **ENCODER SENSOR MOUNT** | DATE: | **5/27/15** |
| PF/SA NO.: | **PF-391-524-98**  | INSPECTOR: | **K. CABAN** |
| WORK ORDER NO.: | **31787-54** | ENGINEER: | **S. GUILLET** | EXT.: | **4771** |
| VENDOR | **BT LASER** | ROUTE TO: | **-** |

|  |  |
| --- | --- |
| **Reason for Non-Compliance:** | **Disposition (UAI, Rework, Scrap, Other):** |

1. , .073 wide slots we not masked, see photo below.
	1. .073 +.001/-.000 are within tolerance even with anodizing (.0735)
	