NON-COMPLIANCE REPORT # 32970-2

|  |  |  |  |
| --- | --- | --- | --- |
| PART NAME: | **3S DRIFT PUMP CAN (TOP HALF ONLY)** | DATE: | **4/6/16** |
| PF/SA NO.: | **PF-444-412-23 R0** | INSPECTOR: | **K. CABAN** |
| WORK ORDER NO.: | **32970-2** | ENGINEER: | **J. VARGAS** | EXT.: |  |
| VENDOR | **MFD** | PLANNER: | **BILL** |

|  |  |
| --- | --- |
| **Reason for Non-Compliance:** | **Disposition (UAI, Rework, Scrap, Other):** |

1. 6.00 ±0.01 tapers from 6.022 - 6.038 (+.012” to + .028” oversized)

2. 6.25 ±0.01 tapers from 6.260 - 6.281 (up to +.021” oversized)

*\*\*Inspection is for Top part only. Part is a remake (32811-2)-which was not QC’d by SLAC Metrology.*