NON-COMPLIANCE REPORT # M-24901

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| PART NAME: | **X-BAND HYBRID FLANGE FEMALE** | DATE: | **8/4/15** | | |
| PF/SA NO.: | **SK-NW-150331-1** | INSPECTOR: | **K. CABAN** | | |
| WORK ORDER NO.: | **M-24901** | ENGINEER: | **N. WHYNOTT** | EXT.: |  |
| VENDOR | **EDM DEPT INC.** | ROUTE TO: | **CUSTOMER** | | |

|  |  |
| --- | --- |
| **Reason for Non-Compliance:** | **Disposition (UAI, Rework, Scrap, Other):** |

1. Dim #6,  of is out of position ranging from 0.0022 to 0.0027 on SN 101 & 102.
2. Dim #20,  measures 0.0678 on SN 101.
3. Dim #46  measures 0.0078 on SN 102.
4. Dim #61,  measures 0.0008 on SN 101.
5. Dim #66,  measures 0.0058 to 0.0065 on SN 101 & 102.

\*\* A. HAASE TOOK SN 103 PRIOR TO MEASUREMENT ON 07/16/15